<ul><li>Protection of the frame, engine and fairing</li><li>Well-shaped, exchangeable (if needed) slider pad made of abrasion-resistant polyamide</li><li>Large contact surface for best possible force distribution</li><li>Optimized surface with good gliding properties</li><li>Extremely solid, CNC-milled substructure made of aluminum alloy</li><li>Easy mounting and sturdy frame attachment thanks to bike-specific add-on elements</li></ul><p><br></p><p><span style="font-weight: bold;">Included in delivery</span>:</p><ul><li>2 x Crash pad</li><li>2 x Mounting bracket</li><li>Mounting instructions</li><li>Mounting material</li></ul><p><br></p><p><span style="font-weight: bold;">Details</span>:</p><ul><li>Material: PA6 Ertalon / Steel</li><li>Surface: powder coated</li><li>Color: black / black</li><li>Weight: 1,0 kg / 2.3 lb</li></ul>