<p>Striking system helmet with a tough and robust appearance and 180° rotatable child part. Fully approved according to the latest strict test standard ECE R2206</p><ul><li>HRT (High Resistant Thermoplastic)</li><li>With ECE R2206 approval and P/J homologation</li><li>180 gr. rotatable chin part hinges to the back of the helmet</li><li>Scale in 2 shell sizes</li><li>Pinlock prepared visor</li><li>Integrated UV resistant sun visor</li><li>Including Pinlock 70 lens</li><li>Airoh logo on the front in tone-in-tone color (black on black)</li><li>1690g. +/- 50g.</li><li>Removable and washable liner and cheek pads</li><li>Microlock chin closure</li></ul>