<p>Overland Fuel Jerrycan for mounting on Kriega OS Platform. The Jerrycans have a specially designed leak-proof neck and threaded cap locking and fuel-resistant gasket for a seamless sealing of the cap.</p><p><span style="font-weight: bold;">Specifications</span>:</p><ul><li>Dimensions: 360 x 270 x 85 mm (W x L x H)</li><li>Capacity: 4.5 liters / 1.19 US gallons</li><li>Weight (incl. spout) empty: 1.1 kg / 2.42 lbs</li><li>Weight (incl. spout) filled 4.5L fuel: 4.4 kg / 9. 72 lbs (based on 1 Dutch petrol liter = 0.737 kilograms)</li><li>Spout: includes Overland-Fuel self-venting spout</li><li>FKM Fuel resistant rubber seal</li><li>Type of fluids: fuel only - Gasoline, diesel, kerosene, gas oil<br><br></li></ul><p>BEFORE USE: Wash thoroughly and allow to dry.</p>